flashrom v0.9.3-r1225 on MS-DOS 7 (i686), built with libpci 3.1.5, GCC 4.3.2, little endian
flashrom is free software, get the source code at http://www.flashrom.org

Calibrating delay loop... OK.
Found "Silicon Image SiI 3114 [SATALink/SATARaid] SATA Ctrl" (1095:3114, BDF 00:08.0).
Warning: Flash seems unconnected.
No EEPROM/flash device found.
Note: flashrom can never write if the flash chip isn't found automatically.
